*** TEST 8 ***
TA1 - task_mode - ASR                  - previous mode:     16#0#
TA1 - task_mode - NO_ASR               - previous mode:     16#0#
TA1 - task_mode - NO_ASR               - previous mode:   16#400#
TA1 - task_mode - ASR                  - previous mode:   16#400#
TA1 - task_mode - NO_TIMESLICE         - previous mode:     16#0#
TA1 - task_mode - TIMESLICE            - previous mode:     16#0#
TA1 - task_mode - TIMESLICE            - previous mode:   16#200#
TA1 - task_mode - NO_TIMESLICE         - previous mode:   16#200#
TA1 - task_mode - PREEMPT              - previous mode:     16#0#
TA1 - task_mode - NO_PREEMPT           - previous mode:     16#0#
TA1 - task_mode - NO_PREEMPT           - previous mode:   16#100#
TA1 - task_mode - PREEMPT              - previous mode:   16#100#
TA1 - task_mode - INTERRUPT_LEVEL( 3 ) - previous mode:     16#0#
TA1 - task_mode - INTERRUPT_LEVEL( 5 ) - previous mode:     16#3#
TA1 - task_mode - set all modes        - previous mode:     16#5#
TA1 - task_mode - set all modes        - previous mode:   16#703#
TA1 - task_mode - clear all modes      - previous mode:   16#703#
TA1 - task_mode - get current mode     - previous mode:     16#0#
*** END OF TEST 8 ***
