*** TEST 16 ***
TA1 - region_ident - rnid => 16#10001#
TA1 - region_get_segment - wait on 100 byte segment from region 2
TA1 - got segment from region 2 - 16#F78#
TA1 - region_get_segment - wait on 3K segment from region 3
TA1 - got segment from region 3 - 16#3F8#
TA1 - region_get_segment - get 3080 byte segment from region 1 - NO_WAIT
TA1 - got segment from region 1 - 16#378#
TA1 - task_wake_after - yield processor
TA2 - region_get_segment - wait on 2K segment from region 1
TA3 - region_get_segment - wait on 3968 byte segment from region 2
<pause>
TA1 - region_return_segment - return segment to region 1 - 16#378#
TA1 - region_get_segment - wait 10 seconds for 3K segment from region 1
TA2 - got segment from region 1 - 16#7F8#
TA2 - region_return_segment - return segment to region 1 - 16#7F8#
TA2 - task_set_priority - make self highest priority task
TA2 - region_get_segment - wait on 3968 byte segment from region 2
TA1 - got segment from region 1 - 16#3F8#
TA1 - region_return_segment - return segment to region 2 - 16#F78#
TA2 - got segment from region 2 - 16#8#
TA2 - region_return_segment - return segment to region 2 - 16#8#
TA2 - task_delete - delete self
TA1 - task_wake_after - yield processor
TA3 - got segment from region 2 - 16#8#
TA3 - region_get_segment - wait on 2K segment from region 3
TA1 - task_delete - delete TA3
<pause>
TA1 - task_wake_after - yield processor
TA4 - region_get_segment - wait on 1.5K segment from region 1
TA5 - region_get_segment - wait on 1.5K segment from region 1
TA1 - region_return_segment - return segment to region 1 - 16#3F8#
TA1 - task_wake_after - yield processor
TA4 - got and returned 16#9F8#
TA5 - got and returned 16#3F0#
TA1 - region_get_segment - wait 10 seconds for 3K segment from region 1
TA1 - got segment from region 1 - 16#3F8#
TA1 - task_wake_after - sleep 1 second
TA4 - region_get_segment - wait on 3K segment from region 1
TA5 - region_get_segment - wait on 3K segment from region 1
TA1 - task_delete - delete TA4
TA1 - region_return_segment - return segment to region 1 - 16#3F8#
TA1 - task_wake_after - yield processor
TA5 - got segment from region 1 - 16#3F8#
TA5 - region_return_segment - return segment to region 1 - 16#3F8#
TA5 - task_delete - delete self
TA1 - region_delete - delete region 1
*** END OF TEST 16 ***
