*** TEST 14 ***
TA1 - signal_catch - INTERRUPT_LEVEL( 3 )
TA1 - signal_send - SIGNAL_16 to self
ASR - ENTRY - signal => 16#10000#
ASR - EXIT  - signal => 16#10000#
TA1 - signal_send - SIGNAL_0 to self
ASR - ENTRY - signal =>     16#1#
ASR - task_wake_after - yield processor
TA2 - signal_send - SIGNAL_17 to TA1
TA2 - task_wake_after - yield processor
ASR - ENTRY - signal => 16#20000#
ASR - EXIT  - signal => 16#20000#
ASR - EXIT  - signal =>     16#1#
TA1 - signal_catch - NO_ASR
<pause>
TA1 - signal_send - SIGNAL_1 to self
ASR - ENTRY - signal =>     16#2#
ASR - task_wake_after - yield processor
TA2 - signal_send - SIGNAL_18 and SIGNAL_19 to TA1
TA2 - task_wake_after - yield processor
ASR - EXIT  - signal =>     16#2#
ASR - ENTRY - signal => 16#C0000#
ASR - EXIT  - signal => 16#C0000#
TA1 - task_mode - disable ASRs
TA1 - sending signal to SELF from timer
TA1 - waiting for signal to arrive
TA1 - timer routine got the correct arguments
TA1 - task_mode - enable ASRs
ASR - ENTRY - signal => 16#8#
ASR - EXIT  - signal => 16#8#
TA1 - signal_catch - ASR ADDRESS of NULL
TA1 - task_delete - delete self
*** END OF TEST 14 ***
