*** TEST 14 ***
TA1 - rtems_signal_catch - RTEMS_INTERRUPT_LEVEL( 3 )
TA1 - rtems_signal_send - RTEMS_SIGNAL_16 to self
ASR - ENTRY - signal => 00010000
ASR - EXIT  - signal => 00010000
TA1 - rtems_signal_send - RTEMS_SIGNAL_0 to self
ASR - ENTRY - signal => 00000001
ASR - rtems_task_wake_after - yield processor
TA2 - rtems_signal_send - RTEMS_SIGNAL_17 to TA1
TA2 - rtems_task_wake_after - yield processor
ASR - ENTRY - signal => 00020000
ASR - EXIT  - signal => 00020000
ASR - EXIT  - signal => 00000001
TA1 - rtems_signal_catch - RTEMS_NO_ASR
<pause>
TA1 - rtems_signal_send - RTEMS_SIGNAL_1 to self
ASR - ENTRY - signal => 00000002
ASR - rtems_task_wake_after - yield processor
TA2 - rtems_signal_send - RTEMS_SIGNAL_18 and RTEMS_SIGNAL_19 to TA1
TA2 - rtems_task_wake_after - yield processor
ASR - EXIT  - signal => 00000002
ASR - ENTRY - signal => 000c0000
ASR - EXIT  - signal => 000c0000
TA1 - rtems_task_mode - disable ASRs
TA1 - sending signal to RTEMS_SELF from timer
TA1 - waiting for signal to arrive
TA1 - timer routine got the correct arguments
TA1 - rtems_task_mode - enable ASRs
ASR - ENTRY - signal => 00000008
ASR - EXIT  - signal => 00000008
TA1 - rtems_signal_catch - asraddr of NULL
TA1 - rtems_task_delete - delete self
*** END OF TEST 14 ***
